*Manufacturer`s name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

*Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

*Phone: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

*E-mail: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

|  |
| --- |
|  |
|  |
|  |

**MANUFACTURER`S DECLARATION**

We hereby declare that the vehicle parts/equipment specified in this declaration are approved and meet the requirements of the respective UN Regulations or EU Directives (Regulation).

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |
| --- | --- |
| *No.* |  |

 | *Name of the part/ equipment* |

|  |  |
| --- | --- |
| *Trademark(s)* |  |

 | *Number of UN Regulation or EU Directive (Regulation)* |
| 1 | Headlamps emitting an asymmetrical passing-beam and/or a driving-beam and equipped with filament lamps of categories R2 and/or HS1 |  | UN Regulation No. 1 |
| 2 | Retro-reflecting devices for power-driven vehicles and their trailers |  | UN Regulation No. 3 |
| 3 | Devices for the illumination of rear registration plates of power-driven vehicles and their trailers |  | UN Regulation No. 4 |
| 4 | "Sealed beam" headlamps (SB) emitting a European asymmetrical passing-beam or a driving-beam or both |  | UN Regulation No. 5 |
| 5 | Direction indicators for power-driven vehicles and their trailers |  | UN Regulation No. 6 |
| 6 | Front and rear position lamps, stop-lamps and end-outline marker lamps for motor vehicles and their trailers |  | UN Regulation No. 7 |
| 7 | Headlamps emitting an asymmetrical passing-beam or a driving-beam or both and equipped with halogen filament lamps (H1, H2, H3, HB3, HB4, H7, H8, H9, HIR1, HIR2 and/or H11) |  | UN Regulation No. 8 |
| 8 | Safety-belts, restraint systems, child restraint systems and ISOFIX child restraint systems for occupants of power-driven vehicles |  | UN Regulation No. 16 |
| 9 | Power-driven vehicle front fog lamps |  | UN Regulation No. 19 |
| 10 | Headlamps emitting an asymmetrical passing-beam or a driving-beam or both and equipped with halogen filament lamps (H4 lamps) |  | UN Regulation No. 20 |
| 11 | Protective helmets and their visors for drivers and passengers of motor cycles and mopeds |  | UN Regulation No. 22 |
| 12 | Reversing and manoeuvring lamps for power-driven vehicles and their trailers |  | UN Regulation No. 23 |
| 13 | Advance-warning triangles |  | UN Regulation No. 27 |
| 14 | Audible warning devices and of motor vehicles with regard to their audible warning signals |  | UN Regulation No. 28 |
| 15 | Pneumatic tyres for motor vehicles and their trailers |  | UN Regulation No. 30 |
| 16 | Halogen sealed-beam headlamps (HSB) emitting a European asymmetrical passing-beam or a driving-beam or both |  | UN Regulation No. 31 |
| 17 | Filament light sources for use in approved lamps of power-driven vehicles and of their trailers |  | UN Regulation No. 37 |
| 18 | Rear fog lamps for power-driven vehicles and their trailers |  | UN Regulation No. 38 |
| 19 | Safety glazing materials and their installation on vehicles |  | UN Regulation No. 43 |
| 20 | Restraining devices for child occupants of power-driven vehicles ("Child Restraint Systems") |  | UN Regulation No. 44 |
| 21 | Devices for indirect vision and of motor vehicles with regard to the installation of these devices |  | UN Regulation No. 46 |
| 22 | Front position lamps, rear position lamps, stop lamps, direction indicators and rear-registration-plate illuminating devices for vehicles of category L |  | UN Regulation No. 50 |
| 23 | Pneumatic tyres for commercial vehicles and their trailers |  | UN Regulation No. 54 |
| 24 | Mechanical coupling components of combinations of vehicles |  | UN Regulation No. 55 |
| 25 | Headlamps for mopeds and vehicles treated as such |  | UN Regulation No. 56 |
| 26 | Headlamps for motor cycles and vehicles treated as such |  | UN Regulation No. 57 |
| 27 | Rear underrun protective devices (RUPDs) |  | UN Regulation No. 58 |
| 28 | Replacement silencing systems |  | UN Regulation No. 59 |
| 29 | Special warning lamps for power-driven vehicles and their trailers |  | UN Regulation No. 65 |
| 30 | Specific equipment of vehicles of category M and N using liquefied petroleum gases in their propulsion system |  | UN Regulation No. 67 |
| 31 | Rear marking plates for slow-moving vehicles (by construction) and their trailers |  | UN Regulation No. 69 |
| 32 | Rear marking plates for heavy and long vehicles |  | UN Regulation No. 70 |
| 33 | Motor cycle headlamps emitting an asymmetrical passing-beam and a driving-beam and equipped with halogen lamps (HS1 lamps) |  | UN Regulation No. 72 |
| 34 | Lateral protection devices (LPD) |  | UN Regulation No. 73 |
| 35 | Pneumatic tyres for L-category vehicles |  | UN Regulation No. 75 |
| 36 | Headlamps for mopeds emitting a driving-beam and a passing-beam |  | UN Regulation No. 76 |
| 37 | Rear-view mirrors of two-wheeled power-driven vehicles with or without side car, with regard to the mounting of rear-view mirrors on handlebars |  | UN Regulation No. 81 |
| 38 | Moped headlamps equipped with filament halogen lamps (HS2) |  | UN Regulation No. 82 |
| 39 | Daytime running lamps for power-driven vehicles |  | UN Regulation No. 87 |
| 40 | Replacement brake lining assemblies, drum-brake linings and discs and drums for power-driven vehicles and their trailers |  | UN Regulation No. 90 |
| 41 | Side-marker lamps for motor vehicles and their trailers |  | UN Regulation No. 91 |
| 42 | Non-original replacement exhaust silencing systems (NORESS) for vehicles of categories L1, L2, L3, L4 and L5 with regard to sound emission |  | UN Regulation No. 92 |
| 43 | Headlamps equipped with gas-discharge light sources |  | UN Regulation No. 98 |
| 44 | Gas-discharge light sources for use in approved lamps of power-driven vehicles |  | UN Regulation No. 99 |
| 45 | Replacement pollution control devices for power-driven vehicles contents |  | UN Regulation No. 103 |
| 46 | Retro-reflective markings for vehicles of category M, N and O |  | UN Regulation No. 104 |
| 47 | Specific components of motor vehicles using compressed natural gas (CNG) and/or liquefied natural gas (LNG) in their propulsion system |  | UN Regulation No. 110 |
| 48 | Motor vehicle headlamps emitting an asymmetrical passing-beam or a driving-beam or both and equipped with filament lamps and/or Light-Emitting Diode (LED) modules |  | UN Regulation No. 112 |
| 49 | Motor vehicle headlamps emitting a symmetrical passing-beam or a driving-beam or both and equipped with filament, gas-discharge light sources or LED modules |  | UN Regulation No. 113 |
| 50 | I Specific LPG (liquefied petroleum gases) retrofit systems to be installed in motor vehicles for the use of LPG in their propulsion systemII. Specific CNG (compressed natural gas) retrofit systems to be installed in motor vehicles for the use of CNG in their propulsion system |  | UN Regulation No. 115 |
| 51 | Tyres with regard to rolling sound emissions and/or to adhesion on wet surfaces and/or to rolling resistance |  | UN Regulation No. 117 |
| 52 | Cornering lamps for power-driven vehicles |  | UN Regulation No. 119 |
| 53 | Adaptive front-lighting systems (AFS) for motor vehicles |  | UN Regulation No. 123 |
| 54 | Enhanced Child Restraint Systems (ECRS) |  | UN Regulation No. 129 |

 *This declaration is issued for the need of regulating vehicle spare parts, and equipment import to Bosnia and Herzegovina for sale and cannot be used for other purposes.*

***Note: Please delete UN Regulations/EU Directive (Regulation) for which the declaration does not apply.***

Place: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ *\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (Place for stamp) Name, surname and signature

of responsible person